## Reporting + (07-07 19:47:52.318)
## Camera Hal Service (camerahalserver pid:821 64BIT) user-build ## fd:10 options(#0) =
  ICameraProviderCallback 0xb4000071ff2f3f50 {.pid = 789, .ptr = 0, .arch = IS_64BIT}
## Camera device manager (since 07-06 17:18:37.760) ##
  Physical Devices: # 2
    [00] -> orientation(wanted/setup)=( 90/90 ) BACK  hasFlashUnit:0 SENSOR_DRVNAME_SC501CS_LYCN_I_MIPI_RAW [PhysEnumDevice:0xb40000719f30d850]
    [01] -> orientation(wanted/setup)=(270/270) FRONT hasFlashUnit:0 SENSOR_DRVNAME_GC02M1_MIPI_RAW [PhysEnumDevice:0xb40000719f30ef30]
  Virtual Devices: # 2
    [device@3.6/internal/0] -> 00 torchModeStatus:NOT_AVAILABLE hasFlashUnit:0 [VirtEnumDevice:0xb40000717f313f50 IVirtualDevice:0xb4000071cf2f0010]
    [device@3.6/internal/1] -> 01 torchModeStatus:NOT_AVAILABLE hasFlashUnit:0 [VirtEnumDevice:0xb40000717f329490 IVirtualDevice:0xb4000071cf2f0e80]
  Open Devices: # 0 (multi-opened maximum: # 1)

################################################################################
## 07-06 17:18:38.560 (1)
## ICameraDevice
## Camera device [0]
## Camera device [device@3.6/internal/0]

== state transition (most recent at bottom): Camera device ==
  07-06 17:18:38.507 : -> initialized
  07-06 18:55:52.387 : -> open +
  07-06 18:55:52.416 : -> open - OK
  07-06 18:55:52.475 : -> constructDefaultRequestSettings (type:0x1) +
  07-06 18:55:52.475 : -> constructDefaultRequestSettings (type:0x1) -
  07-06 18:55:52.500 : -> configure (operationMode:0) +
  07-06 18:55:53.106 : -> configure (operationMode:0) - OK
  07-06 18:55:53.267 : -> 1st request - OK
  07-06 18:55:55.275 : -> flush +
  07-06 18:55:55.307 : -> flush - OK
  07-06 18:55:55.320 : -> configure (operationMode:0) +
  07-06 18:55:55.374 : -> configure (operationMode:0) - OK
  07-06 18:55:56.324 : -> flush +
  07-06 18:55:56.360 : -> flush - OK
  07-06 18:55:56.361 : -> close +
  07-06 18:55:56.449 : -> close - OK

== error state (most recent at bottom): App Stream Manager ==
  [no events yet]

== warning state (most recent at bottom): App Stream Manager ==
  07-06 18:55:55.298 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:56 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 18:55:55.298 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:56 streamId:0x100000027 App:Meta:DynamicP2
  07-06 18:55:55.298 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:56 streamId:0 s0:d0:App:YV12:0|HW_TEXTURE|HW_COMPOSER state:IN-FLIGHT->ERROR
  07-06 18:55:55.298 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:56 streamId:0x1 s1:d0:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 18:55:55.298 : W [0-FrameHandler::updateCallback] requestNo:56 Request Error
  07-06 18:55:55.298 : W [0-FrameHandler::updateCallback] requestNo 56 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 18:55:55.299 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:57 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 18:55:55.300 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:57 streamId:0x100000027 App:Meta:DynamicP2
  07-06 18:55:55.300 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:57 streamId:0 s0:d0:App:YV12:0|HW_TEXTURE|HW_COMPOSER state:IN-FLIGHT->ERROR
  07-06 18:55:55.300 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:57 streamId:0x1 s1:d0:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 18:55:55.300 : W [0-FrameHandler::updateCallback] requestNo:57 Request Error
  07-06 18:55:55.300 : W [0-FrameHandler::updateCallback] requestNo 57 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 18:55:55.300 : W [0-ResultHandler::enqueResult] requestNo:60 existed in mResultQueue[1] - hasLastPartial:0->0
  07-06 18:55:55.301 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:58 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 18:55:55.301 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:60 streamId:0x100000024 App:Meta:DynamicP1_main1
  ...
  07-06 18:55:55.302 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:60 streamId:0 s0:d0:App:YV12:0|HW_TEXTURE|HW_COMPOSER state:IN-FLIGHT->ERROR
  07-06 18:55:55.302 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:60 streamId:0x1 s1:d0:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 18:55:55.302 : W [0-FrameHandler::updateCallback] requestNo:60 Request Error
  07-06 18:55:55.302 : W [0-ResultHandler::enqueResult] requestNo:58 existed in mResultQueue[0] - hasLastPartial:0->1
  07-06 18:55:55.302 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:58 streamId:0x100000027 App:Meta:DynamicP2
  07-06 18:55:55.302 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:58 streamId:0 s0:d0:App:YV12:0|HW_TEXTURE|HW_COMPOSER state:IN-FLIGHT->ERROR
  07-06 18:55:55.302 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:58 streamId:0x1 s1:d0:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 18:55:55.302 : W [0-FrameHandler::updateResult] requestNo:60 is not in FrameQueue; FrameQueue: 58 59; ResultQueue: 58 60
  07-06 18:55:55.302 : W [0-FrameHandler::updateCallback] requestNo:58 Request Error
  07-06 18:55:55.302 : W [0-FrameHandler::updateCallback] requestNo 58 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 18:55:55.303 : W [0-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:59 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 18:55:55.304 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:59 streamId:0 s0:d0:App:YV12:0|HW_TEXTURE|HW_COMPOSER state:IN-FLIGHT->ERROR
  07-06 18:55:55.304 : W [0-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:59 streamId:0x1 s1:d0:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 18:55:55.304 : W [0-FrameHandler::updateCallback] requestNo:59 Request Error
  07-06 18:55:55.304 : W [0-FrameHandler::updateCallback] requestNo 59 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 18:55:55.304 : W [0-FrameHandler::updateCallback] requestNo 60 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 18:55:56.447 : W [0:DeviceSessionPolicy::destroy] not implement yet.

== debug state (most recent at bottom): App Stream Manager ==
  07-06 18:55:55.302 : D [0-FrameHandler::updateResult] requestNo 58, real time:0, last partial:1
  07-06 18:55:55.303 : D [0-FrameHandler::prepareCallbackIfPossible] requestNo:59 Result Error Pending
  07-06 18:55:55.304 : D [0-FrameHandler::updateStreamBuffer] Mark buffer_error. requestNo 59, streamId 0
  07-06 18:55:55.304 : D [0-FrameHandler::updateStreamBuffer] Mark buffer_error. requestNo 59, streamId 1
  07-06 18:55:55.304 : D [0-FrameHandler::updateResult] Empty FrameQueue:0xb40000721f35ba30 0xb40000721f35b990
  07-06 18:55:55.322 : D [0:DeviceSessionPolicy::onEvaluateConfiguration] [hidldc] in->requestedConfiguration=0x7071d26f30, out->resultConfiguration=0x7071d26f18, out->pipelineCfgParams=0x7071d25bc8
  07-06 18:55:55.324 : D [0:DeviceSessionPolicy::onEvaluateConfiguration] [hidldc] out->imageConfigMap->size()=1, out->metaConfigMap->size()=1
  07-06 18:55:55.374 : D [setConfigMap] [debug] imageConfigMap.size()=1, metaConfigMap.size()=1
  07-06 18:55:55.374 : D [0-FrameHandler::setConfigMap] [debug] imageConfigMap.size()=1, metaConfigMap.size()=1
  07-06 18:55:55.374 : D [0-FrameHandler::setConfigMap] [debug] mImageConfigMap.size()=1
  07-06 18:55:56.447 : D [0:DeviceSessionPolicy::~DeviceSessionPolicy] destructor of devicesessionpolicy
  07-06 18:55:56.447 : [destroy] join +
  07-06 18:55:56.447 : D [0-ResultHandler::requestExit] + 0-ResultHandler
  07-06 18:55:56.447 : D [0-ResultHandler::requestExit] - 0-ResultHandler
  07-06 18:55:56.447 : [destroy] join -
  07-06 18:55:56.447 : [destroy] 0:AppMgr-ResCbHelper->join +
  07-06 18:55:56.447 : D [0:AppMgr-ResCbHelper::requestExit] + 0:AppMgr-ResCbHelper
  07-06 18:55:56.447 : D [0:AppMgr-ResCbHelper::requestExit] - 0:AppMgr-ResCbHelper
  07-06 18:55:56.447 : D [0:AppMgr-ResCbHelper::threadLoop] Queue1 is empty
  07-06 18:55:56.447 : [destroy] 0:AppMgr-ResCbHelper->join -
  07-06 18:55:56.447 : [destroy] 0:AppMgr-MsgCbHelper->join +
  07-06 18:55:56.447 : D [0:AppMgr-MsgCbHelper::requestExit] + 0:AppMgr-MsgCbHelper
  07-06 18:55:56.447 : D [0:AppMgr-MsgCbHelper::requestExit] - 0:AppMgr-MsgCbHelper
  07-06 18:55:56.447 : D [0:AppMgr-MsgCbHelper::threadLoop] Queue1 is empty
  07-06 18:55:56.447 : [destroy] 0:AppMgr-MsgCbHelper->join -

################################################################################
## 07-06 17:18:38.562 (1)
## ICameraDevice
## Camera device [1]
## Camera device [device@3.6/internal/1]

== state transition (most recent at bottom): Camera device ==
  07-06 17:18:38.548 : -> initialized
  07-06 17:37:55.628 : -> open +
  07-06 17:37:55.669 : -> open - OK
  07-06 17:37:55.730 : -> constructDefaultRequestSettings (type:0x1) +
  07-06 17:37:55.734 : -> constructDefaultRequestSettings (type:0x1) -
  07-06 17:37:55.760 : -> configure (operationMode:0) +
  07-06 17:37:55.987 : -> configure (operationMode:0) - OK
  07-06 17:37:56.135 : -> 1st request - OK
  07-06 17:37:57.122 : -> flush +
  07-06 17:37:57.136 : -> flush - OK
  07-06 17:37:57.137 : -> close +
  07-06 17:37:57.206 : -> close - OK

== error state (most recent at bottom): App Stream Manager ==
  [no events yet]

== warning state (most recent at bottom): App Stream Manager ==
  07-06 17:37:57.126 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:26 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 17:37:57.127 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:26 streamId:0x100000027 App:Meta:DynamicP2
  07-06 17:37:57.128 : W [1-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:26 streamId:0 s0:d1:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 17:37:57.128 : W [1-FrameHandler::updateCallback] requestNo:26 Request Error
  07-06 17:37:57.128 : W [1-FrameHandler::updateCallback] requestNo 26 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 17:37:57.128 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:27 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 17:37:57.129 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:27 streamId:0x100000027 App:Meta:DynamicP2
  07-06 17:37:57.129 : W [1-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:27 streamId:0 s0:d1:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 17:37:57.129 : W [1-FrameHandler::updateCallback] requestNo:27 Request Error
  07-06 17:37:57.129 : W [1-FrameHandler::updateCallback] requestNo 27 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 17:37:57.130 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:28 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 17:37:57.132 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:28 streamId:0x100000027 App:Meta:DynamicP2
  07-06 17:37:57.132 : W [1-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:28 streamId:0 s0:d1:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 17:37:57.132 : W [1-FrameHandler::updateCallback] requestNo:28 Request Error
  07-06 17:37:57.132 : W [1-FrameHandler::updateCallback] requestNo 28 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  ...
  07-06 17:37:57.132 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:30 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 17:37:57.132 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:29 streamId:0x100000024 App:Meta:DynamicP1_main1
  07-06 17:37:57.133 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:30 streamId:0x100000027 App:Meta:DynamicP2
  07-06 17:37:57.133 : W [1-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:30 streamId:0 s0:d1:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 17:37:57.133 : W [1-FrameHandler::updateCallback] requestNo:30 Request Error
  07-06 17:37:57.133 : W [1-FrameHandler::operator()] [Meta Stream Buffer] Error happens... - requestNo:29 streamId:0x100000027 App:Meta:DynamicP2
  07-06 17:37:57.134 : W [1-FrameHandler::operator()] [Image Stream Buffer] Error happens and all users release - requestNo:29 streamId:0 s0:d1:App:YCrCb_420_SP:0|SW_READ_OFTEN state:IN-FLIGHT->ERROR
  07-06 17:37:57.134 : W [1-FrameHandler::updateCallback] requestNo:29 Request Error
  07-06 17:37:57.134 : W [1-FrameHandler::updateCallback] requestNo 29 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 17:37:57.134 : W [1-FrameHandler::updateCallback] requestNo 30 is removed before shutter callbacked, there MUST have error frames or meta be sent for the request
  07-06 17:37:57.204 : W [1:DeviceSessionPolicy::destroy] not implement yet.

== debug state (most recent at bottom): App Stream Manager ==
  07-06 17:37:57.132 : D [1-FrameHandler::updateResult] requestNo 28, real time:0, last partial:1
  07-06 17:37:57.132 : V [1-FrameHandler::updateCallback] stop updating frame => requestNo: this(29) > latest(28) 
  07-06 17:37:57.132 : D [1-FrameHandler::prepareCallbackIfPossible] requestNo:30 Result Error Pending
  07-06 17:37:57.132 : D [1-FrameHandler::prepareCallbackIfPossible] requestNo:29 Result Error Pending
  07-06 17:37:57.132 : D [1-FrameHandler::prepareCallbackIfPossible] requestNo:30 Result Error Pending
  07-06 17:37:57.133 : D [1-FrameHandler::updateStreamBuffer] Mark buffer_error. requestNo 30, streamId 0
  07-06 17:37:57.133 : D [1-FrameHandler::updateResult] requestNo 30, real time:0, last partial:1
  07-06 17:37:57.133 : D [1-FrameHandler::prepareCallbackIfPossible] requestNo:29 Result Error Pending
  07-06 17:37:57.133 : D [1-FrameHandler::updateStreamBuffer] Mark buffer_error. requestNo 29, streamId 0
  07-06 17:37:57.134 : D [1-FrameHandler::updateResult] requestNo 29, real time:0, last partial:1
  07-06 17:37:57.204 : D [1:DeviceSessionPolicy::~DeviceSessionPolicy] destructor of devicesessionpolicy
  07-06 17:37:57.204 : [destroy] join +
  07-06 17:37:57.204 : D [1-ResultHandler::requestExit] + 1-ResultHandler
  07-06 17:37:57.204 : D [1-ResultHandler::requestExit] - 1-ResultHandler
  07-06 17:37:57.204 : [destroy] join -
  07-06 17:37:57.204 : [destroy] 1:AppMgr-ResCbHelper->join +
  07-06 17:37:57.204 : D [1:AppMgr-ResCbHelper::requestExit] + 1:AppMgr-ResCbHelper
  07-06 17:37:57.204 : D [1:AppMgr-ResCbHelper::requestExit] - 1:AppMgr-ResCbHelper
  07-06 17:37:57.204 : D [1:AppMgr-ResCbHelper::threadLoop] Queue1 is empty
  07-06 17:37:57.204 : [destroy] 1:AppMgr-ResCbHelper->join -
  07-06 17:37:57.204 : [destroy] 1:AppMgr-MsgCbHelper->join +
  07-06 17:37:57.204 : D [1:AppMgr-MsgCbHelper::requestExit] + 1:AppMgr-MsgCbHelper
  07-06 17:37:57.204 : D [1:AppMgr-MsgCbHelper::requestExit] - 1:AppMgr-MsgCbHelper
  07-06 17:37:57.205 : D [1:AppMgr-MsgCbHelper::threadLoop] Queue1 is empty
  07-06 17:37:57.205 : [destroy] 1:AppMgr-MsgCbHelper->join -

################################################################################
## 07-06 17:37:55.653 (1)
## NSCam::v3::pipeline::model::IPipelineModelManager
## IPipelineModelManager: has # 2 IPipelineModel

## IPipelineModel [00]
{.openId=0, .sensorId={0 }, .sensorRawType={0 }}
{.mLogLevel=0, .mHalDeviceAdapter=0xb4000071df2fef50}
{.mUserName=, .mCallback=0x0, .mvOpenFutures#=0, .mSession=0x0}

== error state (most recent at bottom) ==
  [no events yet]

== warning state (most recent at bottom) ==
  [no events yet]

== debug state (most recent at bottom) ==
  [no events yet]


## IPipelineModel [01]
{.openId=1, .sensorId={1 }, .sensorRawType={0 }}
{.mLogLevel=0, .mHalDeviceAdapter=0xb4000071df2fded0}
{.mUserName=, .mCallback=0x0, .mvOpenFutures#=0, .mSession=0x0}

== error state (most recent at bottom) ==
  [no events yet]

== warning state (most recent at bottom) ==
  [no events yet]

== debug state (most recent at bottom) ==
  [no events yet]



################################################################################
## 07-06 17:18:35.818 (0)
## NSCam::ULog
Dump time: 07-07 19:47:52.345519
Flushed!

################################################################################
## 07-06 17:18:40.654 (0)
## NSCam::v3::IStreamInfoPluginManager
Registered Plugin(s):
{ .pluginId=P1STT .options=1 .variantData<1> } [libmtkcam_streaminfo_plugin-p1stt.so 1:0x59b9358fbd9d6e33]

################################################################################
## 07-06 17:37:55.651 (0)
## NSCam::IIonDeviceProvider
## Use shared ion device fd by default?(N), max fd limit:(soft/hard)=(32768/32768)
## Shared ion device fd=-1 (usercount=0)
  07-06 17:37:55.844 fd=37(shared?N) IonHeap-TSF_RingBuf_0
  07-06 17:37:55.844 fd=39(shared?N) IonHeap-TSF_RingBuf_1
  07-06 17:37:55.845 fd=41(shared?N) IonHeap-TSF_RingBuf_2
  07-06 17:37:55.845 fd=43(shared?N) IonHeap-TSF_RingBuf_3
  07-06 18:55:53.049 fd=45(shared?N) IonHeap-TSF_RingBuf_0
  07-06 18:55:53.050 fd=47(shared?N) IonHeap-TSF_RingBuf_1
  07-06 18:55:53.050 fd=49(shared?N) IonHeap-TSF_RingBuf_2
  07-06 18:55:53.050 fd=52(shared?N) IonHeap-TSF_RingBuf_3

################################################################################
## 07-06 17:37:55.828 (0)
## NSCam::IImageBufferHeapManager
  07-06 17:37:55.844 cost(us):  241 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_0 heap-id:[ 38 ] buf{stride/size/pa/va}:[ (1536 24576 04800000 736c3c6000) ] ion{fd/handle/size/pa/va}:[ (38/0x1 24576 04800000 736c3c6000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):82
      #lock:1 usage:0x60033
      07-06 17:37:55.844 10242 TSF_RingBuf_0
  07-06 17:37:55.844 cost(us):   94 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_1 heap-id:[ 40 ] buf{stride/size/pa/va}:[ (1536 24576 04900000 736c3c0000) ] ion{fd/handle/size/pa/va}:[ (40/0x1 24576 04900000 736c3c0000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):38
      #lock:1 usage:0x60033
      07-06 17:37:55.845 10242 TSF_RingBuf_1
  07-06 17:37:55.845 cost(us):   81 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_2 heap-id:[ 42 ] buf{stride/size/pa/va}:[ (1536 24576 04a00000 736c3ba000) ] ion{fd/handle/size/pa/va}:[ (42/0x1 24576 04a00000 736c3ba000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):33
      #lock:1 usage:0x60033
      07-06 17:37:55.845 10242 TSF_RingBuf_2
  07-06 17:37:55.845 cost(us):   82 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_3 heap-id:[ 44 ] buf{stride/size/pa/va}:[ (1536 24576 04b00000 736c3b4000) ] ion{fd/handle/size/pa/va}:[ (44/0x1 24576 04b00000 736c3b4000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):35
      #lock:1 usage:0x60033
      07-06 17:37:55.845 10242 TSF_RingBuf_3
  07-06 18:55:53.049 cost(us):  245 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_0 heap-id:[ 46 ] buf{stride/size/pa/va}:[ (1536 24576 05c00000 736c376000) ] ion{fd/handle/size/pa/va}:[ (46/0x1 24576 05c00000 736c376000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):68
      #lock:1 usage:0x60033
      07-06 18:55:53.050 15451 TSF_RingBuf_0
  07-06 18:55:53.050 cost(us):   91 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_1 heap-id:[ 48 ] buf{stride/size/pa/va}:[ (1536 24576 05d00000 736c370000) ] ion{fd/handle/size/pa/va}:[ (48/0x1 24576 05d00000 736c370000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):27
      #lock:1 usage:0x60033
      07-06 18:55:53.050 15451 TSF_RingBuf_1
  07-06 18:55:53.050 cost(us):   63 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_2 heap-id:[ 50 ] buf{stride/size/pa/va}:[ (1536 24576 05e00000 736c346000) ] ion{fd/handle/size/pa/va}:[ (50/0x1 24576 05e00000 736c346000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):22
      #lock:1 usage:0x60033
      07-06 18:55:53.050 15451 TSF_RingBuf_2
  07-06 18:55:53.050 cost(us):   65 #strong:2-1     1536x16   STA_BYTE(0x2400) IonHeap TSF_RingBuf_3 heap-id:[ 53 ] buf{stride/size/pa/va}:[ (1536 24576 05f00000 736c340000) ] ion{fd/handle/size/pa/va}:[ (53/0x1 24576 05f00000 736c340000) ] offset:[ 0 ] boundary:[ 0 ] contiguousPlanes:N ion-cost(us):24
      #lock:1 usage:0x60033
      07-06 18:55:53.050 15451 TSF_RingBuf_3

################################################################################
## 07-06 17:37:55.946 (0)
## NSCam::v3::NSPipelineContext::IPipelineContextManager

################################################################################
## 07-06 17:37:57.184 (0)
## NSCam::IGenericContainerManager
The number of container map: #0

################################################################################
## 07-06 17:18:35.818 (-1)
## debug
---
## Reporting done - (07-07 19:47:52.371)
